2025 Order Form

**Please read all the terms of the quote and fill out the highlighted sections before signing and submitting it on the form on our website.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Part Name | Number Of Pieces | Piece Price | Lead-Time  Business Days | **# of Parts** | **Coating Type** |
| Full Helmet Assembled | 1-9 | $150 Matte/ $160 Chrome/ $160 Chrome Color/ $220 Two Color Chrome | 5 |  |  |
| Full Helmet Assembled | 10+ | $130 Matte/ $140 Chrome/ $150 Chrome Color/ $210 Two Color Chrome | 10 per 10 |  |  |
| Shell Only | 1-9 | $90 Matte/ $100 Chrome/ $110 Chrome Color/ $140 Two Color Chrome | 5 |  |  |
| Shell Only | 10+ | $80 Matte/ $90 Chrome/ $100 Chrome Color/ $130 Two Color Chrome | 10 per 10 |  |  |
| Face Mask w/ or/ w/o chin attached | 1-9 | $50 Matte/ $60 Chrome/ $70 Chrome Color/ $100 Two Color Chrome | 5 |  |  |
| Face Mask w/ or/ w/o chin attached | 10+ | $40 Matte/ $50 Chrome/ $60 Chrome Color/ $90 Two Color Chrome | 10 per 10 |  |  |
| Visor | 1-9 | $30 Matte/ $35 Chrome/ $40 Chrome Color/ $60 Two Color Chrome | 5 |  |  |
| Visor | 10+ | $20 Matte/ $30 Chrome/ $35 Chrome Color/ $55 Two Color Chrome | 10 per 10 |  |  |
| Chin | 1-9 | $30 Matte/ $35 Chrome/ $40 Chrome Color/ $60 Two Color Chrome | 5 |  |  |
| Chin | 10+ | $20 Matte/ $30 Chrome/ $35 Chrome Color/ $55 Two Color Chrome | 10 per 10 |  |  |
| Clips and Screws  With Helmet Orders | 1-49 | $1.50 Matte/ $2.00 Chrome  $2.50 Chrome Color | 10 |  |  |
| Clips and Screws  With Helmet Orders | 50+ | $1.00 Matte/ $1.50 Chrome  $2.00 Chrome Color | 10 per 50 |  |  |
| Head | 1-9 | $45Matte  $50Chrome  $60 Chrome Color  $70 Fade Chrome / Color  $90 Two Tone / 2 Colors | 5 |  |  |
| Head | 10+ | $40 Matte  $45Chrome  $50 Chrome Color  $60 Fade Chrome / Color  $80 Two Tone / 2 Colors | 10 per 10 |  |  |
| Goalie Head | 1-9 | $55 Matte  $60 Chrome  $65 Chrome Color  $75 Fade Chrome / Color  $90 Two Tone / 2 Colors | 5 |  |  |
| Goalie Head | 10+ | $50 Matte  $55 Chrome  $60 Chrome Color  $65 Fade Chrome / Color  $80 Two Tone / 2 Colors | 10 per 10 |  |  |
| **TOTAL NUMBER OF PARTS** | | |  | | |
| **TENTATIVE PRICE** | | |  | | |

**PRICING IS BASED ON QUANTITY PER FINSIH.**

**EXAMPLE:** 5 CHROME HELMETS, 4 GOLD HELMETS, AND 2 RED HELMETS WOULD BE CHARGED AT THE 1-9 PRICE 10 CHROME HELMETS WOULD BE CHARGED AT THE 10 + PRICE

**All orders must be sent with parts individually bagged and labeled with the desired finish**

##### WARNING! Reconditioning any helmets, masks, or helmet components, sticks, heads, or any other products made by Schutt, Riddell, Warrior, Brine, Cascade, Baur, Xenith, Easton or any other manufacturer of sporting equipment, will void the manufacturers warranty. Mueller Coatings does not offer aftermarket warranty on helmets. Please see the attached safety warnings that are provided with your helmet upon purchase. We will reject any helmet that does not meet our standards for customization. That being, any cracks, holes not applied by OEM, deep cuts or gashes, warped visor and shell, and rusted or rotted face masks. All rivets, screws, and snaps must be in place in firm position before the helmet can be customized. The process used on the helmets is quality tested, patented and trademarked by our vendor. Using vacuum metalizing and painting we produce chrome, gold, colored chrome, and matte decorative looks. These finishes do not have the same durability and/or corrosive resistance that Chrome Plating/ Electroplating has. Testing of durability is the responsibility of the customer. When applying Gold, Colors, and Matte Finishes shading may vary slightly from part to part. There is no warranty on this product it is indented for trophy purposes only

##### Pricing & Payment Terms

Once you submit your order sheet, a representative from Mueller Coatings will be in touch to process your payment and provide a shipping address.

Prices and production rates are subject to change if not quoted with a physical part. We require a 5% reject allowance. Parts will be packed in original containers supplied by you and approved by Mueller Coatings. Packaging will be decided upon and approved before parts are shipped and may affect the price. All incoming containers must be labeled with part description and quantity.

##### Lead Time

Upon receipt of the job an evaluation will occur. Actual lead-time may change after the job is evaluated. You will be notified immediately if lead-time changes. If once we start the job there are contaminants or problems fixturing the job the lead-time may also change. You will be notified immediately if this occurs.

Mueller Coatings processes 5 days per week excluding holidays and will be operating at limited capacity between the Christmas and New Year Holiday season. Notices for the days of operation will be sent 6 weeks prior. This quote is subject to change if not accepted within 30 days.

##### Part(s) Preparation

**Please read this entire section to properly prepare your parts before sending them in.**

All parts must be free of grease, oil, adhesives, or any other contaminants, which will interfere with our metalizing process.

The process uses a basecoat to build a coating for the metalizing to adhere to. All parts must be free of mold release, grease, oil, adhesives, or any other contaminants, which will interfere with our coating processes. These contaminants may affect the adhesions and/or the appearance of the coating. cast resign parts that are cast with a silicone mold or with silicone mold release must be cleaned and primed and/or sealed before we receive them or our coating will separate due to the silicone contamination.

\*Due to the nature of hand masking, there may be deviations from print requirements. If the parts require exact print masking, they are to be masked by the customer prior to the metalizing process. Samples may also be masked at Mueller Coatings, processed, and shipped for approval in writing, which may require signing and returning the sample part(s).

##### Coating Disclosure

There is a certain amount of debris inherent in the process due to dust and debris in the air.

The coating smoothness quality depends on surface finish, if a smooth finish is required the parts must be smooth to start. Any scratches, dings, blisters, or texture, mold lines, imperfection, etc in the part will show through the coating. Any 3D printed, cast, machined, or other manufacturing methods that require secondary finish a filled and sanded 1500 grit or better surface finish is recommended.

The finish should not be pressure washed, cleaned with any chemicals. It will discolor or dull over time if exposed to high temperatures or harsh environments. It will eventually wear or chip. Cleaning should only be performed with a soft cloth and warm water with joy soap.

##### Using vacuum metalizing and paint we produce chrome, gold, colored chrome, and matte decorative looks. These finishes do not have the same durability and/or corrosive resistance that Chrome Plating/ Electroplating has. Testing of durability is the responsibility of the customer. Testing of reflectivity, shielding thickness, and shielding effectiveness is the responsibility of the customer. When applying Gold, Colors, and Matte Finishes shading may vary slightly from lot to lot.

**Shipping Terms**

All freight is F.O.B. our plant. Please note any shipment received without paperwork may delay production until proper paperwork has been received. Please ensure all deliveries have a packing slip attached securely to the outside of one of the packages in the shipment. Mueller Coating’s Receiving personnel do not open and inspect every box upon receipt.


##### There is no warranty on this product it is intended for trophy purposes only

Sincerely yours, Upon acceptance of this quote

Please sign and return with purchase order

MUELLER COATINGS

Company:



Name:

GLENN MUELLER

Signature:

PRESIDENT & CEO

Date:

